Procedural Notes “ Hose Handling “

Operations Manager

CALCO CONCRETE PUMPING INC.

HOSE INSPECTION

Inside Inner diameter degraded

Such as cords showing

Coupling worn on inside

Outside Cords showing

Coupling worn

Hooking up hoses

Use proper size clamp and gasket 2.5” & 4”

Gasket Placement

Flat side to outside

Grooved side to inside.

Place gasket on hose

Place the hose and gasket in clamp.

Place the other hose in clamp.

Close clamp and pin clamp.

Lifting hoses

Lift with your legs not your back.

Roll hose onto your shoulder.